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PEM® Fasteners for Printed Circuit Board Applications
Enable Secure and Reliable Attachment Using Minimal Hardware

Several dedicated families of PEM® fasteners from PennEngineering® enable secure and reliable attachment for a wide range of printed circuit board applications.  Depending on type and style, these fastener solutions can satisfy component-to-board, board-to-board, board-to-chassis, or stacking or spacing attachment challenges.  They offer practical alternatives to loose hardware and other joining methods, install permanently without secondary operations, and ultimately can simplify and streamline assembly.

PEM ReelFast® surface mount fasteners include threaded or unthreaded nuts and standoffs, captive panel screws (spring-loaded or standard), and R’ANGLE® types uniquely providing strong re-usable threads at right angles to boards.  All are supplied on tape and reel compatible with existing SMT automated installation equipment and mount in the same manner and at the same time as other surface mount components prior to the automated reflow solder process.

PEM broaching fasteners include threaded nuts, threaded or unthreaded standoffs, panel fastener assemblies, threaded studs, and SNAP-TOP® standoffs with a spring action to hold boards securely without screws or threaded hardware.  All can be used in boards and in aluminum, acrylic, casting, and polycarbonate components.  During installation, a specially formed axial groove in the fastener broaches into the host material to create a firm, interference-type fit resistant to rotation.

PEM broach/flare-mount standoffs for stacking or spacing applications integrate a combined broach/flare feature promoting even greater pullout performance upon installation in board materials.

The board-oriented product line has further expanded with PEM SpotFast® clinch/broach fasteners ideally suiting applications where metal must be joined to boards or plastic panels.

Detailed specifications and performance data (Bulletin K), fastener drawings, and models can be accessed at www.pemnet.com.

Headquartered in Danboro, PA, USA, and founded in 1942, PennEngineering is a global leader in the fastening industry with technical and manufacturing facilities in North America, Europe, and Asia supported by a global engineering-focused sales force and a worldwide network of authorized distributors.




About Penn Engineering
Penn Engineering & Manufacturing Corp. founded in 1942 in Doylestown, Pennsylvania, USA is the global leader in the design and manufacture of thin sheet fastening devices and installation systems.   The Company is the developer and the sole manufacturer of PEM® brand self-clinching, broaching, surface mount, weld and other 
fasteners.   The Company has manufacturing and technical facilities in two U.S. locations, Galway, Ireland and Kunshan, China. Together they support a network of exclusive global distributors and engineering representatives, providing customers with consistent quality, local sourcing, and technical expertise anywhere in the world.    www.pemnet.com

****Ends****

For sales or marketing information, contact Liam Foy, Director of Marketing EMEA, PennEngineering, tel: +353 91 7471186 e-mail: lfoy@pemnet.com


For media information, contact Debbie Norton, Senior Account Manager, Napier, 
tel: +44 (0) 1243 531123 mob: + 44 (0) 7818 064176 email: debbie@napierb2b.com 
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